Follow these steps to install SES-DACC Software



1. Install FT-232 Driver.

2. Run SETUP.EXE given in setup folder.

3. MS Power Pack is given in power pack folder. Install the required files from here as required by the software during installaion. 

4. Now setup is ready to perform experiment.


For any assistance contact below address:

SES Instruments Pvt. Ltd.,
452, Adarsh Nagar, Roorkee-247 667, U.K. (INDIA)
Phone : +91-1332-272852, 277118, Fax: 277118,
Email: info@sesinstruments.com, www.sesinstruments.com